**To,**

**…………………………………………………………………………….**

**…………………………………………………………………………….**

**…………………………………………………………………………….**

**Subject :- Repair of roof slab of class rooms at ground floor ,reconstruction of roof slab of class rooms & verandah at first floor and front elevation work in college .**

**Dear Sir,**

The quotations are invited in sealed envelope by undersigned for the subject work on dated 30 -04-2025 at 11.00 A.M. in undersigned’ s office as per schedule enclosed herewith .

You are advised to visit at site in college days / time for any enquiry before submitting the quotation .

Thanks .

For Champa Agarwal Inter College

( PRINCIPAL)

**SCHEDULE OF QUANTITY**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SNo.** | **Description of Item** | **Qty.** | **Unit** | **Rate** | **Amount** |
| 1. | Dismantling of existing flooring of 1st Floor rooms and after replacement of damaged/missing stones flooring is to be done by using necessary earth , old available bricks / new bricks , grouting with cement mortar 1 : 4 ( 1 cement : 4 chambal sand ) complete. | 2400 | Sq.f t. |  |  |
| **2.** | Replacement of damaged/missing red sand stone of roof slab of gr. Floor with cement mortar. | 250 | Sq.ft. |  |  |
| **3.** | Provision of roof slab of 1st floor class rooms & verandah by using steel girder (4 kg/rft ), red sand stone ,earth , new bricks ,grouting and plastering with cement mix 1:4 ( 1 cement : 4 chambal sand ). | 4800 | Sq.ft. |  |  |
| **4.** | Parapet wall 4.5” thick and 2’-0” high with new 1st class bricks & cement mortar 1:4 ( 1 cement : 4 stone dust ) including plastering 1: 5 ( 1 cement : 5 chambal sand ) complete. | 660 | Sq.ft. |  |  |
| **5.** | Provision of 100 mm. dia, 4 kg/cm2 rain water pipe | 250 | Rft. |  |  |
| **6.** | Provision of R.C.C. pilers in verandah at 1st floor including dismantling of old pilers and casting of new pilers by using necessary shuttering ,reinforcement & R.C.C. 1:2:3 complete . | 10 | Each |  |  |
| **7.** | Front elevation work as per existing block design by dismantling of old brick wall/arch and making with new brick wall ,beam , cement jali & both side plastering etc. complete .(Front area will be measured for payment and no opening of design will be deducted ) | 1100 | Sq.ft. |  |  |
| **8.** | Brick work with new bricks & cement mortar 1 : 6 ( 1 cement : 6 stone dust ) including both side plastering 1:5 ( 1 cement : 5 chambal sand ) wherever required . | 100 | Sq.ft. |  |  |
| **9.** | Repair to old plastering by removing of old plaster and new plastering with 1:5 ( 1 cement : 5 chambal sand ) | 500 | Sq.ft. |  |  |
|  | **G.S.T. WILL BE PAID SEPRATELY AS APPLICABLE** | | | **TOTAL:** |  |
|  |  |  |

**Terms & Conditions Of Quotation :**

**Material to be used :**

1:- Cement : Jk ,Birla Uttam ,Shree PPC Grade

2:- Bricks : 1st Class

**Mode of payment**

All contractors are advised to take running payments during execution as per mutual understanding of both parties however the final payment will be made within 15 days after completion.

**Completion Period 06 months**

**Note :-**

1. Electricity ,water & store for cement &tools will be provided by college free of cost.
2. The rates are for mentioned work only. Extra Work will be paid extra.
3. College administration will be fully responsible for MVDA, NAGARNIGAM etc.
4. The actual area of each & every item will be measured for payment purpose.
5. The contractor will arrange all required material, labour ,T&P ,scaffolding etc. for the execution of the work.
6. The contractor is advised to follow all safety & security measures during execution.