**To,**

**The Principal/ Manager,**

**Champa Agrawal Inter College,**

**Mathura.**

**Subject: - Quotation/ Estimate for renovation work in class rooms & verandah of academic block in college.**

Dear Sir,

We are enclosed herewith our most competitive offer for the subject work as per description given below:

**ONLY STRUCTURE WORK**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SNo.** | **Description of Item** | **Qty.** | **Unit** | **Rate** | **Amount** |
| 1. | Dismantling of existing flooring of 1st Floor rooms and after replacement of damaged/missing stones flooring is to be done by using necessary earth , old available bricks / new bricks , grouting with cement mortar 1 : 4 ( 1 cement : 4 chambal sand ) complete. | 2400 | Sq.f t. | 80/- | 192000 |
| **2.** | Replacement of damaged/missing red sand stone of roof slab of gr. Floor with cement mortar. | 500 | Sq.ft. | 60/- | 30000 |
| **3.** | Provision of roof slab of 1st floor class rooms & verandah by using steel girder (4 kg/rft ), red sand stone ,earth , new bricks ,grouting and plastering with cement mix 1:4 ( 1 cement : 4 chambal sand ). | 4800 | Sq.ft. | 300/- | 1440000 |
| **4.** | Parapet wall 4.5” thick and 2’-0” high with new 1st class bricks & cement mortar 1:4 ( 1 cement : 4 stone dust ) including plastering 1: 5 ( 1 cement : 5 chambal sand ) complete. | 660 | Sq.ft. | 150/- | 99000 |
| **5.** | Provision of 100 mm. dia, 4 kg/cm2 rain water pipe | 250 | Rft. | 140/- | 35000 |
| **6.** | Provision of R.C.C. pilers in verandah at 1st floor including dismantling of old pilers and casting of new pilers by using necessary shuttering ,reinforcement & R.C.C. 1:2:3 complete . | 10 | Each | 5000 | 50000 |
| **7.** | Front elevation work as per existing block design by dismantling of old brick wall/arch and making with new brick wall ,beam , cement jali & both side plastering etc. complete .(Front area will be measured for payment and no opening of design will be deducted ) | 1100 | Sq.ft. | 250/- | 275000 |
| **8.** | Brick work with new bricks & cement mortar 1 : 6 ( 1 cement : 6 stone dust ) including both side plastering 1:5 ( 1 cement : 5 chambal sand ) wherever required . | 100 | Sq.ft. | 200/- | 20000 |
| **9.** | Repair to old plastering by removing of old plaster and new plastering with 1:5 ( 1 cement : 5 chambal sand ) | 1000 | Sq.ft. | 40/- | 40000 |
|  | **G.S.T. WILL BE CHARGED SEPRATELY AS APPLICABLE** | | | **TOTAL:** | **2181000** |
|  |  |  |

**Material to be used :**

1:- Cement : Jk ,Birla Uttam ,Shree PPC Grade

2:- Bricks : 1st Class

**Mode of payment**

We will produce two bills on date 1st & 16th of work done and you are kindly requested to release the payment by 5th & 20th of every month.

**Completion Period 06 months**

**Note :-**

1. Electricity ,water & store for cement &tools will be provided by college free of cost.
2. The rates are for mentioned work only. Extra Work will be charged extra.
3. College administration will be fully responsible for MVDA, NAGARNIGAM etc.

Hoping for favorable reply and assuring you for our best services.

Thanking you Yours Sincerely

(Anuj Kumar Saxena )

( Auth. Signatory)

( For Shree Krishna Construction )